TECHNICAL DETAILS

* Input Voltage: Up to 12V
* LCD Pins: 15(RS), E(4), D4(2), D5(14), D6(13), D7(5)
* TFT 2.4" Pins: TFT\_CS(15), TFT\_RST(4), TFT\_D/C(2), TFT\_MOSI(23), TFT\_SCK(18), TFT\_MISO(19), T\_CLK(18), T\_CS(14), T\_DIN(23), T\_OUT(19), T\_IRQ(13)
* OLED Pins: GND, VCC, SCL, SDA. Make sure the first pin is GND - Some OLEDs has VCC pin as the first pin.
* SD Pins: SD\_CS(5), SD\_MOSI(23), SD\_MISO(19), SD\_SCK(18)
* Neopixel Pin: 16
* Buzzer Pin: 17
* Button Input Pins: 34, 35, 36, 39
* Capacitive Touch Pin: 33
* Dimensions: 100mm x 81mm
* Snapped Dimensions: 56mm x 81mm